**Supplementary data**

Fig. S1. Full wavelength scan of CR

Fig. S2. Standard calibration curve of CR at 495 nm